[image: USY_MB1_RGB_Standard_Logo.tif]
SAFE WORK PROCEDURE


SAFE WORK PROCEDURE
Use this form to document Safe Work Procedures for hazardous activities and processes. The information in your Safe Work Procedure (SWP) should be supported by a risk assessment.  

	Faculty/School:
	School of Physics
	Initial Issue Date: January 2026

	
	
	Next Review Date: January 2027

	SWP Reference Number:
	SWP-A28-SAIL-116C-bambu-h2d
	Version: 1.1
	Version Issue Date: January 2026

	SWP Title:

	Operation of Bambu Lab H2D Laser Edition with 10W Class 4 Laser Module

	Prepared by:

	Chris Betters

	Responsible supervisor/s:

	Chris Betters, Sergio Leon-Saval



	List  the Hazards and risk controls as per risk assessment

	Associated risk assessment reference:
	Hazards
	Risk controls




	RA-A28-SAIL-116C-bambu-h2d
	Class 4 laser radiation (455nm, 10W)
	- Laser safety windows and interlocks
- NEVER operate with safety systems defeated
- Mandatory training and competency assessment

	RA-A28-SAIL-116C-bambu-h2d
	Fire and ignition
	- Fire detection and emergency stop
- NEVER leave unattended during laser operations
- CO₂ or dry powder fire extinguisher within 5 metres

	RA-A28-SAIL-116C-bambu-h2d
	Thermal burns (350°C nozzle, 65°C chamber)
	- Heat-resistant gloves for hot surfaces
- Cool-down period before handling components

	RA-A28-SAIL-116C-bambu-h2d
	Inhalation of fumes and particulates
	- Local exhaust ventilation
- Enclosed build chamber and Smoke Purifier filtration

	RA-A28-SAIL-116C-bambu-h2d
	Electrical hazards (240V)
	- RCD protection and earthed equipment
- Regular test and tag; no wet conditions

	RA-A28-SAIL-116C-bambu-h2d
	Moving mechanical parts
	- Enclosed design with door interlocks
- Emergency stop accessible; keep hands clear during operation

	RA-A28-SAIL-116C-bambu-h2d
	Toxic fumes from certain materials
	- Material approval process; prohibited materials list enforced
- Local exhaust ventilation



	List resources required including personal protective clothing, chemicals and equipment needed



PERSONAL PROTECTIVE EQUIPMENT (PPE):
- Heat-resistant gloves (for handling hot components after printing)
- Safety glasses (general workshop protection, NOT for laser - the laser safety windows provide laser protection)
- Respiratory protection (if required based on material SDS and ventilation assessment)
- Closed-toe shoes
- Long trousers (no shorts)
- Tie back long hair
EQUIPMENT AND MATERIALS:
- Bambu Lab H2D with 10W laser module (fully functional with all safety systems verified)
- Approved materials only (wood, leather, acrylic, etc. - see approved materials list)
- Material Safety Data Sheets (SDS) for all materials to be processed
- Bambu Studio or Bambu Suite software (latest version)
- Computer with network connection
- Clean, lint-free cloths for maintenance
- Isopropyl alcohol (IPA) for cleaning
SAFETY EQUIPMENT (MUST BE PRESENT IN LABORATORY):
- CO₂ or dry powder fire extinguisher (within 5 metres)
- First aid kit
- Emergency eyewash station (accessible)
- Emergency contact numbers displayed
- Sign-in/sign-out log book
VENTILATION:
- Local exhaust ventilation (LEV) connected and operating
- Air purifier (recommended for prolonged use)
- Exhaust ducting to outside or through appropriate filtration


	List step by step instructions or order for undertaking the task


BEFORE STARTING - CRITICAL SAFETY REQUIREMENTS:
- You must have completed Class 4 laser safety training and been assessed as competent
- You must be listed on the authorised users list for this equipment
- You must never leave the equipment unattended during laser operations
- You must never defeat or bypass any safety system
PRE-OPERATION SAFETY CHECKS (MANDATORY - DO NOT SKIP):
Sign in to the equipment log book (record name, date, time, operation type)
Visual inspection of laser safety windows:
- Check front laser safety window (green-tinted) for cracks, chips, or damage
- Check all side panels and top cover for damage
- If ANY damage found: DO NOT USE - lock out and report to supervisor
Test door interlocks (CRITICAL):
- Power on the equipment
- Navigate to settings menu and initiate a test print or laser operation
- Slowly open the front door - laser/print head MUST stop immediately
- Close door and repeat test with top glass cover
- If interlocks fail: DO NOT USE - lock out and report immediately
Emergency stop test:
- Press the red emergency stop button
- Verify all motion stops and alarm sounds
- Reset emergency stop by twisting clockwise
Verify local exhaust ventilation (LEV):
- Check exhaust ducting is connected
- Turn on LEV/air purifier
- Verify airflow (use tissue test if needed)
Check fire extinguisher:
- CO₂ or dry powder extinguisher present within 5 metres
- Check pressure gauge in green zone
- Check clear access path to extinguisher
Clear work area:
- Remove all flammable materials from vicinity (papers, solvents, etc.)
- Ensure clear egress path for emergency evacuation
- Remove clutter around equipment
MATERIAL PREPARATION AND APPROVAL:
Check material is approved:
- Consult approved materials list
- PROHIBITED: PVC, polycarbonate, materials containing chlorine or halogens
- If material not on approved list: seek approval from supervisor before use
Review material Safety Data Sheet (SDS):
- Check for hazardous decomposition products
- Note any special ventilation or PPE requirements
- Confirm fire hazards and extinguishing methods
Prepare material:
- Ensure material is clean and dry
- Check material dimensions fit within build volume (350 × 320 × 325 mm for 3D printing, 310 × 270 mm for laser engraving with 10W module)
- For laser operations: ensure material is flat and securely positioned
EQUIPMENT STARTUP:
Power on the Bambu H2D (if not already on from safety checks)
Allow equipment to complete startup sequence and homing
Check touchscreen display for any error messages
Verify network connection (if remote monitoring to be used)
Start LEV/air purifier system
PREPARE JOB FILE:
Open Bambu Studio or Bambu Suite software on computer
Import or create your design file
For 3D printing:
- Select material type and printer settings
- Configure support structures if needed
- Slice the model and preview toolpaths
- Check estimated print time and material usage
For laser engraving/cutting:
- Use BirdsEye camera to align material on bed
- Set laser power and speed for material type (consult manufacturer guidelines)
- Configure air assist settings
- Preview laser path
- Verify material will not extend outside safe area
Send job file to printer via network or USB
LOAD MATERIAL:
Open front door (equipment should be idle, not during operation)
For 3D printing:
- Clean build plate with IPA if needed
- Install appropriate build plate (textured PEI, smooth PEI, etc.)
- Load filament spools into AMS (if using multi-material)
- Verify filament type matches job requirements
For laser operations:
- Remove build plate if necessary
- Position material on bed using alignment guides
- Use BirdsEye camera to verify material position
- Ensure material is flat and won't curl during processing
- Verify material is within safe operating area
Close front door securely - ensure door clicks closed
START OPERATION:
Final check before starting:
- All doors and covers closed and secured
- LEV/air purifier running
- Emergency stop not engaged
- Fire extinguisher accessible
- Clear path to emergency exit
Select job from touchscreen or send from computer
Confirm job parameters on screen
Press start button
Monitor first few minutes closely:
- Watch for proper adhesion (3D printing) or correct laser focus (laser operations)
- Listen for unusual sounds
- Watch for excessive smoke or fumes
- Verify material not moving or curling
During laser operations - MANDATORY ATTENDANCE:
- You MUST remain within visual line of sight OR monitor via camera continuously
- Never leave the room during laser cutting/engraving
- Watch for signs of fire (flames, excessive smoke, burning smell)
- Keep emergency stop and fire extinguisher within reach
- If you must leave for any reason: STOP the laser operation first
During 3D printing operations:
- Check periodically for print failures
- Can be left unattended if print-only mode (no laser)
- Camera monitoring recommended for long prints
COMPLETION AND SHUTDOWN:
Wait for equipment to signal job complete
Allow hot components to cool:
- Nozzle: can reach 350°C - wait minimum 10 minutes
- Chamber: can reach 65°C - wait 5 minutes
- Build plate: wait until below 40°C (touchscreen displays temperature)
Open front door carefully (watch for residual heat)
Remove completed work:
- Wear heat-resistant gloves if components still warm
- For 3D prints: allow to cool on plate before removal
- For laser work: carefully remove material (may have sharp edges)
- Place in designated area for cooling/collection
Clean work area (see Clean Up and Waste Disposal Requirements section)
Turn off LEV/air purifier (after ensuring adequate ventilation time)
If last user of the day: power down equipment via touchscreen menu
Sign out in equipment log book (record time, any issues)


	List emergency shutdown procedures 


EMERGENCY STOP - USE IN ANY OF THESE SITUATIONS:
- Fire or smoke detected
- Any safety system failure
- Equipment malfunction
- Abnormal sounds, smells, or operation
- Laser radiation suspected (door opened during operation)
- Material movement or dislodgement
- Any unsafe condition
EMERGENCY SHUTDOWN PROCEDURE:
1. PRESS RED EMERGENCY STOP BUTTON IMMEDIATELY: button located on front right of equipment; push firmly - button will lock in depressed position; audible alarm will sound; all motion will stop immediately
2. If emergency stop fails or is inaccessible: turn off power at wall outlet; pull plug if necessary
3. Assess the situation: if fire - follow fire emergency procedures; if injury - call for first aid assistance; if equipment damage - do not restart, report to supervisor; if safety system failure - lock out and tag equipment
Do NOT restart equipment until:
- Emergency has been fully resolved
- Equipment has been inspected
- Supervisor has given approval
- Any necessary repairs completed
- All safety systems verified functional
Complete incident report:
- Record time, date, and circumstances
- Note what emergency required shutdown
- Report to supervisor immediately
- Complete RiskWare report if required
RESETTING EMERGENCY STOP (ONLY AFTER EMERGENCY RESOLVED):
1. Ensure all emergency conditions resolved
2. Twist emergency stop button clockwise to release - button will pop up and alarm will stop
3. Equipment will not automatically restart - manual restart required
4. Perform full pre-operation safety checks before resuming work


	List Emergency procedures for how to deal with fires, spills or exposure to hazardous substances 


FIRE EMERGENCY:
- PRESS EMERGENCY STOP BUTTON
- DO NOT OPEN CHAMBER DOOR (introduces oxygen, may worsen fire)
- If fire is small and contained inside chamber: fire detection system will sound alarm; use CO₂ or dry powder fire extinguisher through any access points; direct extinguisher at base of flames; use short bursts; if fire does not extinguish immediately, proceed to evacuation
- If fire cannot be controlled or spreads: evacuate area immediately; close door behind you (do not lock); activate building fire alarm; call 000 (Emergency Services); notify building warden; assemble at designated assembly point; do not re-enter building until cleared by emergency services
- After fire is extinguished: allow equipment to cool completely; do not restart - lock out and tag equipment; report incident to supervisor immediately; complete incident report and RiskWare entry; equipment must be inspected before further use
SUSPECTED LASER RADIATION EXPOSURE:
- PRESS EMERGENCY STOP IMMEDIATELY
- If eye exposure suspected: do not rub eyes; close eyes or look away from bright light; seek IMMEDIATE medical attention at Emergency Department; call 000 if severe symptoms (vision loss, severe pain); Class 4 laser exposure can cause permanent blindness
- If skin exposure (burns): move away from laser source; cool affected area with running cool water for 20 minutes; cover with clean, non-fluffy material; seek medical attention if severe
- Document incident: record time, duration, and circumstances of exposure; note which safety system(s) failed; report immediately to supervisor and safety officer; complete incident report and RiskWare entry
- Equipment must be locked out and tagged immediately, inspected by a qualified laser safety technician, and all safety systems verified before any further use
THERMAL BURNS (HOT SURFACES):
- Remove from heat source immediately
- Cool affected area with running cool water for 20 minutes
- Remove jewellery or tight clothing near burn (unless stuck to skin)
- Cover burn with clean, non-fluffy material (cling film is ideal)
- Seek medical attention if: burn larger than 5 cm across; burn on face, hands, feet, joints, or genitals; full thickness burn (white or charred skin); blistering; or if unsure of severity
- Complete first aid documentation and incident report
EXCESSIVE FUMES OR SMOKE:
- PRESS EMERGENCY STOP
- If fumes are overwhelming: evacuate area immediately; do not inhale deeply; get to fresh air
- When safe to do so: increase ventilation (open doors/windows); continue running LEV/air purifier
- If anyone experiences symptoms (difficulty breathing, dizziness, nausea): call 000 for medical assistance; keep person in fresh air; provide material SDS to medical personnel
- Investigation required: check LEV system connection and function; check material type (may be prohibited); review material SDS for decomposition products; report to supervisor; do not resume until issue resolved
EQUIPMENT MALFUNCTION:
- Press emergency stop
- Isolate power if safe to do so
- Do NOT attempt repairs yourself
- Lock out and tag equipment
- Report to supervisor
- Complete incident report
EMERGENCY CONTACTS:
- Emergency Services: 000
- University Security (after hours): [Insert number]
- Supervisor: Chris Betters [Insert number]
- Safety Officer: [Insert name and number]
- First Aid: [Location and contact details]
- Nearest Emergency Department: [Insert details]


	List Clean up and waste disposal requirements


AFTER EACH USE - BUILD CHAMBER AND SURFACES:
- Allow all components to cool to room temperature before cleaning
- Remove any loose debris, dust, or residue from build chamber
- Use lint-free cloth with isopropyl alcohol (IPA) to clean: build plate; laser safety windows (interior and exterior - ensure no residue that could affect laser protection); front door window; any smoke/dust deposits on internal surfaces
- Do NOT use water or harsh chemicals on electronic components
AFTER EACH USE - LASER OPTICS AND AIR ASSIST (AFTER LASER OPERATIONS):
- Check laser lens for smoke residue or debris
- Clean if necessary using approved lens cleaning materials only
- Check air assist nozzle for blockages
- Clear any debris from air assist system
EXHAUST SYSTEM AND FILTERS:
- Check exhaust system for blockages weekly
- Inspect air filter condition
- Replace filters according to schedule (quarterly or when visibly saturated)
- Clean or replace according to manufacturer guidelines
- Document filter changes in maintenance log
WORK AREA:
- Remove all materials, tools, and personal items
- Dispose of waste properly (see waste disposal below)
- Wipe down surrounding benches
- Return fire extinguisher to proper location if moved
- Leave area clean and tidy for next user
WASTE DISPOSAL - 3D PRINTING WASTE:
- Failed prints, support material: general waste, or recycling if material is recyclable (check material type)
- Filament offcuts: store for potential reuse or dispose in general waste
- Empty filament spools: recycling (plastic recycling bin)
WASTE DISPOSAL - LASER PROCESSING WASTE:
- Wood/paper offcuts: general waste or composting if uncontaminated
- Acrylic offcuts: general waste (not recyclable if laser-cut due to residue)
- Leather offcuts: general waste
- Metal sheet offcuts: metal recycling
- Any waste contaminated with hazardous materials: consult SDS and dispose as hazardous waste if required
WASTE DISPOSAL - CLEANING MATERIALS:
- IPA-contaminated cloths: allow to dry in well-ventilated area, then general waste
- Used filters: sealed bag, then general waste (or hazardous waste if heavily contaminated)
WASTE DISPOSAL - HAZARDOUS WASTE:
- Any material that produced toxic fumes during processing
- Contaminated cleaning materials
- Dispose via university hazardous waste system
- Label clearly and contact waste management
MONTHLY DEEP CLEANING:
- Clean linear guides and lubricate with appropriate lubricant
- Clean lead screws and apply grease
- Vacuum chamber exhaust fan and vents
- Clean part cooling fan and air ducts
- Inspect all moving parts for wear
- Document in maintenance log


	List references used in the development of this SWP, e.g. codes of practice


AS/NZS IEC 60825.1:2014 - Safety of laser products
AS 2211.13-1999 - Safety of industrial laser equipment
Work Health and Safety Act 2011
Work Health and Safety Regulation 2017
AS/NZS 3000:2018 - Electrical installations (Wiring Rules)
AS 1940-2017 - Storage and handling of flammable and combustible liquids
Bambu Lab H2D User Manual (latest version)
Bambu Lab H2D Laser Safety Document (wiki.bambulab.com/en/h2/laser-safety-document)
Bambu Lab H2D Technical Specifications
Risk Assessment RA-A28-SAIL-bambu-h2d
University of Sydney WHS Laser Safety Policy and Procedures
University of Sydney WHS Fire Safety Procedures
Material Safety Data Sheets (SDS) for approved materials


	List competency required – qualifications, certificates, licensing, training - e.g. course or instruction: 


MANDATORY TRAINING 1 - CLASS 4 LASER SAFETY TRAINING (must be completed before authorisation):
- Understanding of laser classifications
- Class 4 laser hazards (eye damage, burns, fire)
- How safety systems work (interlocks, windows)
- Consequences of defeating safety systems
- Emergency procedures for laser exposure
- Legal responsibilities
MANDATORY TRAINING 2 - EQUIPMENT-SPECIFIC TRAINING:
- Bambu H2D operation (3D printing and laser functions)
- Safety system verification procedures
- Pre-operation checks
- Software operation (Bambu Studio/Suite)
- Material preparation and loading
- Emergency stop and shutdown procedures
MANDATORY TRAINING 3 - FIRE SAFETY TRAINING:
- Fire extinguisher operation (CO₂ and dry powder types)
- Fire emergency procedures
- Building evacuation procedures
MANDATORY TRAINING 4 - HAZARDOUS MATERIALS AWARENESS:
- Reading and interpreting SDS
- Prohibited materials (PVC, polycarbonate, etc.)
- Fume hazards and controls
- Material approval process
MANDATORY TRAINING 5 - FIRST AID (BASIC):
- Thermal burns treatment
- When to seek medical attention
- Location of first aid equipment
COMPETENCY ASSESSMENT - THEORY:
- Written test or oral examination covering: Class 4 laser hazards and safety systems; pre-operation safety checks; emergency procedures; prohibited materials; equipment limitations
- Must achieve 100% on safety-critical questions
- Minimum 80% overall pass mark
COMPETENCY ASSESSMENT - PRACTICAL:
- Supervised practical demonstration of: complete pre-operation safety checks (including interlock testing); material preparation and approval process; equipment startup procedure; loading material safely; starting and monitoring a job (3D print or laser operation); emergency stop activation and reset; safe shutdown and cleanup
- Assessor must observe and verify competency in all areas
- Any safety-critical errors require retraining and reassessment
ONGOING REQUIREMENTS:
- Annual refresher training on laser safety
- Retraining required after any safety incident involving this equipment, when safety procedures are updated, if unsafe practices are observed, or after an extended period of non-use (more than 12 months)
- Baseline eye examination recommended before authorisation
- Periodic eye examinations if frequent laser user (consult occupational health)
ASSESSOR REQUIREMENTS (to be authorised as an assessor, staff must):
- Have completed Class 4 laser safety training
- Be competent and experienced in operation of the Bambu H2D
- Understand all safety systems and their verification
- Be familiar with emergency procedures
- Have authority to authorise equipment use
- Be approved by laboratory manager or safety officer
ASSESSMENT PROCESS:
- Trainee completes all mandatory training modules
- Assessor conducts theory assessment (written or oral)
- Assessor supervises practical demonstration and verifies competency in all required areas
- If competent: assessor signs trainee off on sign-off sheet and trainee is added to authorised users list
- If not yet competent: additional training and practice required, then reassessment
AUTHORISED USERS LIST:
- Maintained by laboratory manager and displayed near equipment
- Updated when new users authorised; reviewed annually
- Users removed if required retraining not completed
RECORD KEEPING:
- Training records maintained by supervisor
- Competency assessment documented on sign-off sheet
- Training refresher dates tracked


	Staff approved to assess competence for this SWP


Chris Betters (Supervisor), Sergio Leon-Saval (Supervisor), [Additional authorised assessors to be added]



	SWP Sign off sheet	


	SWP name and version:

	Operation of Bambu Lab H2D Laser Edition with 10W Class 4 Laser Module (Version 1.1)




In signing this section the assessor agrees that the following persons are competent in following this SWP.

	Name
	Signature
	Date Competent
	Name of Assessor/Authoriser
	Assessor/Authoriser signature

	 
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	





Risk Matrix
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